



Nozzle Temp 215

Bed Temp 60





* Change Z-Axis Offsets as needed for your print surface.
* Ignore the baud rate – I don’t connect it via USB to this computer. Set baud to 250000 due to AVR error rates if you print directly via USB

